Checklist – CAC044M
Road Furniture (Steel Beam Guardrail) (MRTS14, MUTCD)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Contractor |  | Date |  | Review No. |  |
| Contract No. |  | Project No. |  | Project Name |  |

| Reference | Requirements | Addressed | Comments/Observations |
| --- | --- | --- | --- |
| Delineators |
| MRTS14Cl 20.4.8 | Delineators shall be installed in the locations and to the spacings as shown on the Standard Drawings. Delineators shall conform to the requirements specified in Clause 10.2.4 of MRTS14. |  |  |
| Installation |
| MRTS14Cl 20.6.2 | Steel posts may be driven or installed by the excavation and backfilling of a post hole. |  |  |
| MRTS14Cl 20.6.2  | During the driving of any post, no damage shall occur to the post or any protective coating. |  |  |
| SD1474 | Has a clear zone been constructed behind the MELT components? |  |  |
| SD1474 | Are end treatments in accordance with specifications? |  |  |

**Additional Issues for consideration**

|  |  |
| --- | --- |
| 1 | Check for underground services location before installing posts. |
| 2 | Are laps on panels facing the correct direction? |

*Delete below section if not required*

|  |  |  |  |
| --- | --- | --- | --- |
| Audited by: |  |  |  |
| Name |  | Signature |  | Date |  |