|  |  |
| --- | --- |
|  |  |
| **Annexure MRTS03.1 (January 2019)** |
| **Drainage, Retaining Structures and Protective Treatments** |
|  |
| **Specific Contract Requirements** |
|  |
| **Contract Number**  |  |
|  |
| Note: | Clause references within brackets in this Annexure refer to Clauses in the parent Technical Specification MRTS03 unless otherwise noted. |

|  |
| --- |
| Testing Frequencies (Clause 5.4)The following minimum testing frequencies and minimum number of tests shall apply to the construction of work covered by this Technical Specification. |

| Construction Activity | Normal Testing level | Reduced testing level |
| --- | --- | --- |
| Minimum testing frequency | Minimum number of tests | Minimum testing frequency | Minimum number of tests |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

|  |
| --- |
| Components to be salvagedCulvert and culvert end structures (Clause 8.2)The following culverts and/or culvert end structures shall be salvaged. |
|  |  |

|  |
| --- |
| Salvage storage location (Clause 8.2)The location of the storage site for salvaged materials is as follows. |
|  |  |

|  |
| --- |
| Supply of Precast and Preformed CulvertHelical lock-seam corrugated aluminium pipe culvert components (Clause 11.2)The following requirements shall apply to the supply of helical lock-seam corrugated aluminium pipe culvert components. |
|  |  |

|  |
| --- |
| Details of precast and preformed culvert components (supply only) (Clause 11.2)Details of any precast and preformed culvert components supplied only under the Contract are as follows. |
| Item number | Description | Section size (mm) | Length (metres) | Class or gauge | Design height of fill (metres)† |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
| **†** For reinforced concrete box culverts only. |

|  |
| --- |
| Fabric-encased concrete batter protection (Clause 44.3.3) |
| The average thickness of the concrete mat shall be |  |

|  |
| --- |
| Interlocking blocks – Approved Products (Clause 48.2)The following products are approved for use as interlocking block protection. |
|  |  |

|  |
| --- |
| Supplementary Requirements (Clause 58)The following supplementary requirements shall apply. |
|  |  |