|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | | |  | |
| **Annexure MRTS08.1 (July 2021)** | | |
| **Plant-Mixed Heavily Bound (Cemented) Pavements** | | |
|  | | |
| **Specific Contract Requirements** | | |
|  | | |
| **Contract Number** | |  |
|  | | | | |
| Note: | Clause references within brackets in this Annexure refer to Clauses in the parent Technical Specification MRTS08 unless otherwise noted. | | | |
| Design Traffic (Clause 6.1.2) | | | |
| |  |  | | --- | --- | | Location | Average Daily Traffic in the Design Lane in Year of Opening –  Equivalent Standard Axles (ESA) | |  |  | |  |  | |  |  | |  |  |   If no indication is given for a particular location, the Administrator shall confirm the average daily traffic in the design lane in year of opening based on advice from the projects pavement designer. | | | |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Construction requirementsPaving equipment (Clause 8.2.1.4) | | | | | |
|  | A self-propelled spreading machine (paver) is required: | Yes |  | No |  |
|  | If no indication is given, a self-propelled spreading machine (that is, a paver) shall be used. | | | | |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Intelligent Construction Rollers (Clause 8.2.1.7) | | | | | |
|  | Intelligent Construction (IC) rollers shall be used to compact heavily bound pavement material: | Yes |  | No |  |
|  | If no indication is given, the rollers to be used shall be nominated by the Contractor in their Heavily Bound Pavement Construction Procedure. | | | | |

|  |
| --- |
| Where IC equipped rollers are not available locally, existing rollers may need to be retrofitted with IC equipment. |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Deviation from a straight-edge (Clause 8.3.6) | | | | | |
|  | The maximum deviation from a straight-edge shall be alternative: | C (5 mm) |  | D (8 mm) |  |
|  | If no indication is given, the maximum deviation from a straight-edge shall be Alternative C. | | | | |

|  |  |  |  |
| --- | --- | --- | --- |
| Road roughness (Clause 8.3.7) | | | |
|  | The maximum road roughness shall be (Rs) |  | m/km |
|  | If no indication is given, the requirement shall be 2.31. | | |

|  |  |  |
| --- | --- | --- |
| Trafficking during construction (Clause 8.2.11) | | |
|  | The following requirements for trafficking during construction shall apply. | |
|  | Layer | Requirement |
|  |  |
|  |  |
|  | If no indication is given, the requirements of Clause 8.2.11 shall apply. | |

|  |  |
| --- | --- |
| Supplementary requirements (Clause 10) | |
|  | The following supplementary requirements shall apply. |
|  |  |