|  |  |
| --- | --- |
|  |  |
| **Annexure MRTS45.1** |
| **Road Surface Delineation** |
|  |
| **Specific Contract Requirements** |
|  |
| **Contract Number**  |  |
|  |
| Note: | Clause references within brackets in this Annexure refer to Clauses in the parent Technical Specification MRTS45 unless otherwise noted. |

|  |
| --- |
| Testing Frequencies (Clause 5.3)The following minimum testing frequencies shall apply to pavement marking. |
| Construction activity | Minimum testing frequency | Minimum number of tests |
| **Materials** |  |  |
| **Thickness of pavement markings** |  |  |
| Longitudinal lines |  |  |
| Transverse markings |  |  |
| **Dimensions of pavement markings (including location)** |  |  |
| Longitudinal lines |  |  |
| Transverse markings |  |  |
| **Dimensions of raised pavement marker placement** |  |  |
| **Dimensions of ATLM** |  |  |
| **Retroreflectivity** |  |  |
| Skid resistance |  |  |
| **Notes**The retroreflectivity of new pavement markings shall be a minimum of 350 mcd/lux/m² when measured up to 20 days after painting (See Clause 6.1.1 MRTS45). |

|  |
| --- |
| Reflective glass beads (Clause 6.1.3)Reflective glass beads shall be as stated below. |
|  | **Type B** |  |

|  |  |  |
| --- | --- | --- |
|  | **Type B-HR** |  |

|  |  |  |
| --- | --- | --- |
|  | **Type C** |  |

|  |  |  |
| --- | --- | --- |
|  | **Type D** |  |

|  |  |  |
| --- | --- | --- |
|  | **Type D-HR** |  |

|  |
| --- |
| Cold applied plastic (Clause 6.1.6)The following supplementary requirements shall apply. |
|  |  |

|  |
| --- |
| Removal of existing pavement markings (Clause 7.10)The following method shall be used for removal of existing pavement markings. |
|  |  |

|  |
| --- |
| Supplementary requirements (Clause 10)The following supplementary requirements shall apply. |
|  |  |