|  |  |
| --- | --- |
|  |  |
| **Annexure MRTS81.1** |
| **Bridge Bearings** |
|  |
| **Specific Contract Requirements** |
|  |
| **Contract Number**  |  |
|  |
| Note: | Clause references within brackets in this Annexure refer to Clauses in the parent Technical Specification MRTS81 unless otherwise noted. |

|  |  |
| --- | --- |
| Structure |  |

|  |
| --- |
| Elastomeric bearings (Clause 6)Single unbonded layer bearingsThe following information is required to be supplied for all single unbounded layer bearings. |
| Standard Work Item Number | Dimensions (mm) | Service load at zero shear and zero rotation (kN/m) |
| Length | Breath | Thickness |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

|  |
| --- |
| Laminated elastomeric bearingsThe following information is required to be supplied for laminated elastomeric bearings. |
| Standard Work Item Number | AS part number (refer AS 5100.4) |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

|  |
| --- |
| Pot bearings (Clause 7)The following information is required to be supplied for all pot bearings. |
| Item No. | Location | Type (sliding or fixed) | Maximum ultimate compression load (kN) | Maximum ultimate shear load (kN) | Minimum ultimate compression load (kN) | Serviceability vertical load (kN) | Movement (sliding bearings) (mm) | Design rotation (radian) |
| ULCmax | ULSmax | ULCmin | SLSmax |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |

|  |
| --- |
| Supplementary requirements (Clause 8)The following supplementary requirements shall apply to the supply and testing of bearings. |
|  |  |