|  |  |
| --- | --- |
|  |  |
| **Annexure MRTS13.1** |
| **Bituminous Slurry Surfacing** |
|  |
| **Specific Contract Requirements** |
|  |
| **Contract Number**  |  |
|  |
| Note: | Clause references within brackets in this Annexure refer to Clauses in the parent Technical Specification MRTS13 unless otherwise noted. |

|  |
| --- |
| Specific Treatments (Clauses 9.2, 9.3.5, 9.6.1 and 9.6.2)The specific treatment(s) for work under this Contract shall be as stated below. |
| Reference Location |  |  |  |  |  |
| Control Line |  |  |  |  |  |
| Section | From |  |  |  |  |  |
| To |  |  |  |  |  |
| Length (m) |  |  |  |  |  |
| Nominal Width (m) |  |  |  |  |  |
| Area (m²) |  |  |  |  |  |
| Preparation Surface Defects Treatment Code †¹ |  |  |  |  |  |
| Surfacing System | Surfacing System †² |  |  |  |  |  |
| Mix Designation (QS) |  |  |  |  |  |
| Thickness (mm) |  |  |  |  |  |
| Surface Texture †³ |  |  |  |  |  |
| Second Application | SurfacingSystem †² |  |  |  |  |  |
| Mix Designation (QS) |  |  |  |  |  |
| Thickness (mm) |  |  |  |  |  |
| Surface Texture †³ |  |  |  |  |  |

†1 Refer to Clause 2 of Annexure MRTS13.1

†² Slurry Seal or Microsurfacing

†³ Standard or hessian (Refer to Clause 9.6.2)

|  |
| --- |
| Preparation of Existing Surface (Clauses 9.3.4 and 9.3.5)Surface defects shall be repaired as stated below. |
| Surface Defect Treatment Code | **A** | **B** | **C** | **D** | **E** |
| Crack Filling † |  |  |  |  |  |
| Pothole Repair † |  |  |  |  |  |
| Repairs to Failed Pavement † |  |  |  |  |  |
| Tack Coat Required † |  |  |  |  |  |
| Tack Coat Application Rate (litres/m²) |  |  |  |  |  |

† Yes or No

|  |
| --- |
| Rut Filling (Clause 9.5)Rut filling shall be carried out as stated below. |
| Rut Filling Treatment Code | Bituminous Slurry Mix Design |
| A |  |
| B |  |
| C |  |
| D |  |

|  |
| --- |
| Supplementary Requirements (Clause 11)The following supplementary requirements shall apply. |
|  |  |