**Checklist – CAC060M  
Inspection – Steel-Reinforced Concrete Pipes – MRTS25**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Contractor** |  | **Date** |  | **Review No.** |  |
| **Contract No.** |  | **Project No.** |  | **Project Name** |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Unit Numbers** |  | **Unit Types** |  | **Date Manufactured** |  |

| Reference | Requirements | Addressed | Comments/Observations |
| --- | --- | --- | --- |
| MRTS25 Cl. 6.1 | Concrete mix |  |  |
| MRTS25 Cl. 6.2 | Reinforcing steel |  |  |
| MRTS25 Cl. 6.3 | Nibs |  |  |
| MRTS25 Cl. 10  AS 4058 Cl. 1.5 | Marking & identification of product |  |  |
| MRTS25 Cl. 7b | Curing |  |  |
| MRTS25 Cl. 7c  AS 4058 Cl. 3.4 | Surface finish |  |  |
| MRTS25 Cl. 7d | Dimensional check  Cover check |  |  |
| MRTS25 Cl. 7d | Water absorption |  |  |
| MRTS25 Cl. 7d | Proof load testing |  |  |
| MRTS25 Cl. 7d | Ultimate load testing |  |  |
| AS 4058 Cl. 3.5 | Stacking and storage |  |  |
|  | Were repairs carried out satisfactorily? |  |  |
| AS 4058 Cl. 3.5 | Loading and transport |  |  |

*Delete below section if not required*

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Audited by: |  | |  | |  | |
| Name |  | Signature |  | Date |  |