Checklist – CAC091M  
Protection of Survey Marks (MRTS56)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Contractor |  | Date |  | Review No. |  |
| Contract No. |  | Project No. |  | Project Name |  |

| Reference | Requirements | Addressed | Comments |
| --- | --- | --- | --- |
| MRTS56  Clause 7.3.3 | Have all the surveying requirements for cadastral reference mark protection been undertaken prior to excavation works for noise fences? Hold Point 4 |  |  |
| MRTS56  Clause 7.3.3 | Have all the surveying requirements for cadastral reference mark protection been undertaken prior to excavation works for retaining walls? Hold Point 5 |  |  |
| MRTS56  Clause 7.3.3 | Have all the surveying requirements for cadastral reference mark protection been undertaken prior to excavation works for earthwork cuttings or trenching works? Hold Point 6 |  |  |
| MRTS56  Clause 7.3.3 | Have all the surveying requirements for cadastral reference mark protection been undertaken prior to removal / demolition of kerbs, kerbs and channel and concrete slabs? Hold Point 7 |  |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Reviewed by: |  | |  | |  | |
| Name |  | Signature |  | Date |  |