|  |  |
| --- | --- |
|  |  |
| **Annexure MRTS110.1 (March 2023)** |
| **Coloured Surface Treatments** |
|  |
| **Specific Contract Requirements** |
|  |
| **Contract Number**  |  |
|  |
| Note: | Clause references within brackets in this Annexure refer to clauses in the parent Technical Specification MRTS110 unless otherwise noted. |

|  |
| --- |
| Site details (Clause 8) |
|  | Location | Existing Pavement Surfacing Type1 | Nominal Length (m) | Nominal Width (m) | Approximate Area (m²) |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  | Note:1 Due to open graded asphalt being a porous road surface, placement of CST over open graded asphalt should be avoided, where possible. |

|  |
| --- |
| Transport and Main Roads Registration Level (Clause 8) |
| The Transport and Main Roads Registration Level for the CST product used in the Works shall be: |  |  |

|  |
| --- |
| * Registration Level 3 is typically specified where a minimum of 5 years satisfactory performance is desired.
* Registration Level 2 is typically specified where a minimum of 2 years satisfactory performance is desired.
* Registration Level 1 is typically specified for small scale, low risk sites.

If no indication is given, Registration Level 2 will apply. |

|  |
| --- |
| Supplementary Requirements (Clause 13) |
|  | The following supplementary requirements shall apply to this Technical Specification. |
|  |  |